jpeg2yuv(1)

NAME
jpeg2yuv - Convert jpeg images to the yuv format.

SYNOPSIS
jpeg2yuv [-b num] [-f num] [-I num] [-A ratio] [-L num] [-n num] [-l num] [-j filename]

DESCRIPTION
jpeg2yuv decompresses a sequence of JPEG files and pipes the image data to stdout as a YUV4MPEG2 stream. Any JPEG format supported by libjpeg can be read. stdout will be filled with the YUV4MPEG2 movie data stream, so be prepared to pipe it on to mpeg2enc or to write it into a file.

OPTIONS
jpeg2yuv accepts the following options:

-b num
    Frame offset: skip output of the first 'num' frames. (default: 0)

-f num
    Set the frame rate of stream accepts the same numbers. No default, this option has to be specified.

-A ratio
    Sample aspect ratio. Default is square pixels (1:1)

-I num
    interlacing mode: p = none / progressive
    t = top field first
    b = bottom field first
    No default, this option has to be specified.

-L num
    0 = non-interlaced (two successive fields per JPEG file)
    1 = interlaced fields

-l num
    Specifies the number of loops (default: 0 loops )
    When this option is not used the given range of images is only processed once. If you use this option with num of -1 jpeg2yuv will loop forever writing the image to stdout. When you use n > 0 it will loop n-times till it finishes.

-n num
    Specifies the number of frames to process. (default: all = -1)

-j {1}%{2}d{3}
    Read JPEG frames with the name components as follows:
     {1} JPEG filename prefix (e g: picture_ )
     {2} Counting placeholder (like in C, printf, eg 06 ))
     {3} File extension. Something like this: .jpg A correct description of the files could look like this: picture_%06d.jpg If this option is omited, the filenames are read from stdin. For example:
     $ls *jpg | jpeg2yuv -f 25 -I p > result.yuv

-R 1 or 0
    rescale YUV color values from 0-255 to 16-235 (default: 1)

-v num
    Verbosity level (0, 1 or 2)

BUGS
The frame rate description seems not to be up to date. The NTSC integer ratios seem not to be supported. As a workaround specify a PAL (25) or FILM (24) and set the right frame rate in mpeg2enc with the -F option.

AUTHOR
This man page was written by Bernhard Praschinger.
If you have questions, remarks, problems or you just want to contact the developers, the main mailing list for the MJPEG-tools is:
  mjpeg-users@lists.sourceforge.net

For more info, see our website at
    http://mjpeg.sourceforge.net

SEE ALSO
mjpegtools(1), mpeg2enc(1), ppmtoy4m(1), yuv2lav(1), yuvdenoise(1), yuvmedianfilter(1), yuvscaler(1)